**Ni foil**

15-05-2020 – Dmitry/..

PETRA III Extension Beamline P65

XAS CONTINUOUS MODE

Chart, line chart

Description automatically generated

E0 = **8333** eV, Edge step = **1.3**, Pre-edge = -150 to -30 eV, Normalization = 50 to 700 eV

Chart, histogram

Description automatically generated kw = 2

Chart, line chart

Description automatically generatedFT k range = 2.2 – 12.5 Å-1