**Rh foil**

03-06-2021 – …../..

PETRA III Extension Beamline P65

XAS CONTINUOUS MODE

Chart, line chart

Description automatically generated

E0 = **23220** eV, Edge step = **1.9**, Pre-edge = -150 to -30 eV, Normalization = 50 to 850 eV

Chart

Description automatically generated kw = 2

Chart, line chart

Description automatically generated FT k range = 2.4 – 15.2 Å-1